// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	compatible = "z-router,zr-2660", "mediatek,mt7621-soc";
	model = "Z-ROUTER ZR-2660";

	aliases {
		label-mac-device = &gmac0;

		led-boot = &led_power_green;
		led-failsafe = &led_power_green;
		led-running = &led_power_green;
		led-upgrade = &led_power_green;
	};

	chosen {
		bootargs = "console=ttyS0,115200";
	};

	keys {
		compatible = "gpio-keys";

		key-0 {
			label = "reset";
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led-0 {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WAN;
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
		};

		led-1 {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WLAN;
			function-enumerator = <50>;
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		led-2 {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_LAN;
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
		};

		led-3 {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WLAN;
			function-enumerator = <24>;
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		led-4 {
			color = <LED_COLOR_ID_RED>;
			function = LED_FUNCTION_WAN;
			gpios = <&gpio 16 GPIO_ACTIVE_HIGH>;
		};

		led_power_green: led-5 {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_POWER;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
		};
	};
};

&gmac0 {
	nvmem-cells = <&macaddr_factory_3fff4>;
	nvmem-cell-names = "mac-address";
};

&gmac1 {
	status = "okay";
	label = "wan";
	phy-handle = <&ethphy4>;

	nvmem-cells = <&macaddr_factory_3fffa>;
	nvmem-cell-names = "mac-address";
};

&ethphy4 {
	/delete-property/ interrupts;
};

&nand {
	status = "okay";

	mediatek,nmbm;
	mediatek,bmt-max-ratio = <1>;
	mediatek,bmt-max-reserved-blocks = <64>;

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		partition@0 {
			label = "u-boot";
			reg = <0x0 0x80000>;
			read-only;
		};

		partition@80000 {
			label = "Config";
			reg = <0x80000 0x80000>;
			read-only;
		};

		partition@100000 {
			label = "factory";
			reg = <0x100000 0x80000>;
			read-only;

			nvmem-layout {
				compatible = "fixed-layout";
				#address-cells = <1>;
				#size-cells = <1>;

				eeprom_factory_0: eeprom@0 {
					reg = <0x0 0xe00>;
				};

				macaddr_factory_4: macaddr@4 {
					compatible = "mac-base";
					reg = <0x4 0x6>;
					#nvmem-cell-cells = <1>;
				};

				macaddr_factory_3fff4: macaddr@3fff4 {
					reg = <0x3fff4 0x6>;
				};

				macaddr_factory_3fffa: macaddr@3fffa {
					reg = <0x3fffa 0x6>;
				};
			};
		};

		partition@180000 {
			label = "firmware";
			reg = <0x180000 0x7680000>;

			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "kernel";
				reg = <0x0 0x400000>;
			};

			partition@400000 {
				label = "ubi";
				reg = <0x400000 0x7280000>;
			};
		};
	};
};

&pcie {
	status = "okay";
};

&pcie1 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;

		mediatek,disable-radar-background;

		nvmem-cells = <&eeprom_factory_0>;
		nvmem-cell-names = "eeprom";

		#address-cells = <1>;
		#size-cells = <0>;

		band@1 {
			reg = <1>;
			nvmem-cells = <&macaddr_factory_4 1>;
			nvmem-cell-names = "mac-address";
		};
	};
};

&state_default {
	gpio {
		groups = "i2c", "jtag", "wdt";
		function = "gpio";
	};
};

&switch0 {
	ports {
		port@1 {
			status = "okay";
			label = "lan1";
		};

		port@2 {
			status = "okay";
			label = "lan2";
		};

		port@3 {
			status = "okay";
			label = "lan3";
		};
	};
};
