/dts-v1/;

#include "ipq5018.dtsi"
#include "ipq5018-ess.dtsi"
#include "ipq5018-qcn6122.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	model = "GL.iNet GL-B3000";
	compatible = "glinet,gl-b3000", "qcom,ipq5018";

	aliases {
		ethernet1 = &dp2;
		label-mac-device = &dp2;
		led-boot = &led_system_blue;
		led-failsafe = &led_status_white;
		led-running = &led_status_white;
		led-upgrade = &led_system_blue;
		serial0 = &blsp1_uart1;
	};

	chosen {
		bootargs-append = " root=/dev/ubiblock0_1 swiotlb=1 coherent_pool=2M";
		stdout-path = "serial0:115200n8";
	};

	keys {
		compatible = "gpio-keys";
		pinctrl-0 = <&button_pins>;
		pinctrl-names = "default";

		button-reset {
			label = "reset";
			gpios = <&tlmm 27 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-0 = <&leds_pins>;
		pinctrl-names = "default";

		led_system_blue: system-blue {
			color = <LED_COLOR_ID_BLUE>;
			function = LED_FUNCTION_STATUS;
			gpios = <&tlmm 24 GPIO_ACTIVE_HIGH>;
		};

		led_status_white: status-white {
			color = <LED_COLOR_ID_WHITE>;
			function = LED_FUNCTION_STATUS;
			gpios = <&tlmm 23 GPIO_ACTIVE_HIGH>;
		};
	};
};

&switch {
	status = "okay";
	switch_mac_mode = <MAC_MODE_SGMII_CHANNEL0>;

	qcom,port_phyinfo {
		// MAC0 -> GE Phy -> QCA8337 Phy2
		port@0 {
			port_id = <1>;
			mdiobus = <&mdio0>;
			phy_address = <7>;
		};

		// MAC1 ---SGMII---> QCA8337 SerDes
		port@1 {
			port_id = <2>;
			forced-speed = <1000>;
			forced-duplex = <1>;
		};
	};
};

// MAC1 ---SGMII---> QCA8337 SerDes
&dp2 {
	status = "okay";
	nvmem-cells = <&macaddr_dp2 0>;
	nvmem-cell-names = "mac-address";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&mdio0 {
	status = "okay";
};

&mdio1 {
	status = "okay";
	pinctrl-0 = <&mdio1_pins>;
	pinctrl-names = "default";
	reset-gpios = <&tlmm 39 GPIO_ACTIVE_LOW>;

	// QCA8337 Phy0 -> WAN
	qca8337_0: ethernet-phy@0 {
		reg = <0>;
	};

	// QCA8337 Phy1 -> LAN1
	qca8337_1: ethernet-phy@1 {
		reg = <1>;
	};

	// QCA8337 Phy3 -> LAN2
	qca8337_2: ethernet-phy@2 {
		reg = <2>;
	};

	// QCA8337 switch
	switch0: ethernet-switch@17 {
		compatible = "qca,qca8337";
		reg = <17>;
		#address-cells = <1>;
		#size-cells = <0>;

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			switch0cpu: port@0 {
				reg = <0>;
				label = "cpu";
				phy-mode = "sgmii";
				ethernet = <&dp2>;
				qca,sgmii-enable-pll;

				fixed-link {
					speed = <1000>;
					full-duplex;
				};
			};

			// QCA8337 Phy0 -> WAN
			port@1 {
				reg = <1>;
				label = "wan";
				phy-handle = <&qca8337_0>;
			};

			// QCA8337 Phy1 -> LAN1
			port@2 {
				reg = <2>;
				label = "lan1";
				phy-handle = <&qca8337_1>;

				nvmem-cells = <&macaddr_dp2 2>;
				nvmem-cell-names = "mac-address";
			};

			// QCA8337 Phy3 -> LAN2
			port@3 {
				reg = <3>;
				label = "lan2";
				phy-handle = <&qca8337_2>;

				nvmem-cells = <&macaddr_dp2 2>;
				nvmem-cell-names = "mac-address";
			};
		};
	};
};

&sleep_clk {
	clock-frequency = <32000>;
};

&xo_board_clk {
	clock-div = <4>;
	clock-mult = <1>;
};

&blsp1_uart1 {
	pinctrl-0 = <&serial_0_pins>;
	pinctrl-names = "default";
	status = "okay";
};

&crypto {
	status = "okay";
};

&cryptobam {
	status = "okay";
};

&prng {
	status = "okay";
};

&qfprom {
	status = "okay";
};

&qpic_bam {
	status = "okay";
};

&qpic_nand {
	pinctrl-0 = <&qpic_pins>;
	pinctrl-names = "default";
	status = "okay";

	nand@0 {
		compatible = "spi-nand";
		reg = <0>;
		nand-ecc-engine = <&qpic_nand>;
		nand-bus-width = <8>;

		partitions {
			compatible = "qcom,smem-part";

			partition-0-art {
				label = "0:art";
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_dp2: macaddr@0 {
						compatible = "mac-base";
						#nvmem-cell-cells = <1>;
						reg = <0x6 0x6>;
					};
				};
			};
		};
	};
};

&tlmm {
	mdio1_pins: mdio-state {
		mdc-pins {
			pins = "gpio36";
			function = "mdc";
			drive-strength = <8>;
			bias-pull-up;
		};

		mdio-pins {
			pins = "gpio37";
			function = "mdio";
			drive-strength = <8>;
			bias-pull-up;
		};
	};

	leds_pins: leds-pins {
		pins = "gpio23", "gpio24";
		function = "gpio";
		drive-strength = <8>;
		bias-pull-down;
	};

	button_pins: button-pins {
		pins = "gpio27";
		function = "gpio";
		drive-strength = <8>;
		bias-pull-up;
	};

	qpic_pins: qpic-state {
		clock-pins {
			pins = "gpio9";
			function = "qspi_clk";
			drive-strength = <8>;
			bias-disable;
		};

		cs-pins {
			pins = "gpio8";
			function = "qspi_cs";
			drive-strength = <8>;
			bias-disable;
		};

		data-pins {
			pins = "gpio4", "gpio5", "gpio6", "gpio7";
			function = "qspi_data";
			drive-strength = <8>;
			bias-disable;
		};
	};

	serial_0_pins: uart0-state {
		pins = "gpio20", "gpio21";
		function = "blsp0_uart0";
		drive-strength = <8>;
		bias-disable;
	};
};

&q6v5_wcss {
	/* B3000 currently doesn't support passing bootargs */
	/*boot-args = <					*/
			/*       type:	0x1  PCIE0	*/
			/*     length:	4		*/
			/*      PD id:	3		*/
			/* reset GPIO:	15		*/
			/*   reserved:	0 0>;		*/
};

&wifi {
	status = "okay";

	qcom,rproc = <&q6_wcss_pd1>;
	qcom,userpd-subsys-name = "q6v5_wcss_userpd1";
	qcom,ath11k-calibration-variant = "GL-iNet-GL-B3000";
	qcom,ath11k-fw-memory-mode = <1>;
	qcom,bdf-addr = <0x4c400000>;
};

&wifi1 {
	status = "okay";

	qcom,rproc = <&q6_wcss_pd3>;
	qcom,userpd-subsys-name = "q6v5_wcss_userpd3";
	qcom,ath11k-calibration-variant = "GL-iNet-GL-B3000";
	qcom,ath11k-fw-memory-mode = <1>;
	qcom,bdf-addr = <0x4d100000>;
	qcom,m3-dump-addr = <0x4df00000>;
};
