// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar7100.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	compatible = "trendnet,tew-673gru", "qca,ar7161";
	model = "TRENDNET TEW-673GRU";

	aliases {
		label-mac-device = &eth1;
		led-boot = &led_wps;
		led-failsafe = &led_wps;
		led-running = &led_wps;
		led-upgrade = &led_wps;
	};

	leds {
		compatible = "gpio-leds";

		led_wps: wps {
			function = LED_FUNCTION_WPS;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&gpio 9 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
		};

		wps {
			label = "wps";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
		};
	};

	rtl8366s {
		compatible = "realtek,rtl8366s";
		gpio-sda = <&gpio 5 GPIO_ACTIVE_HIGH>;
		gpio-sck = <&gpio 7 GPIO_ACTIVE_HIGH>;
		realtek,initvals = <0x06 0x0108>;

		mdio-bus {
			#address-cells = <1>;
			#size-cells = <0>;
			status = "okay";

			phy4: ethernet-phy@4 {
				reg = <4>;
				phy-mode = "rgmii";
			};
		};
	};

	virtual_flash {
		compatible = "mtd-concat";
		devices = <&fwconcat0 &fwconcat1>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x0 0x0>;
			};
		};
	};
};

&usb1 {
	status = "okay";
};

&usb2 {
	status = "okay";
};

&usb_phy {
	status = "okay";
};

&pcie0 {
	status = "okay";

	wifi@11,0 {
		compatible = "pci168c,0029";
		reg = <0x8800 0 0 0 0>;
		nvmem-cells = <&cal_caldata_1000>, <&macaddr_lan 0>;
		nvmem-cell-names = "calibration", "mac-address";
	};

	wifi@12,0 {
		compatible = "pci168c,0029";
		reg = <0x9000 0 0 0 0>;
		nvmem-cells = <&cal_caldata_5000>, <&macaddr_wan 1>;
		nvmem-cell-names = "calibration", "mac-address";
	};
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x040000>;
				read-only;
			};

			partition@40000 {
				label = "config";
				reg = <0x040000 0x010000>;
				read-only;
			};

			fwconcat0: partition@50000 {
				label = "fwconcat0";
				reg = <0x050000 0x610000>;
			};

			partition@660000 {
				label = "caldata";
				reg = <0x660000 0x010000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					cal_caldata_1000: calibration@1000 {
						reg = <0x1000 0xeb8>;
					};

					cal_caldata_5000: calibration@5000 {
						reg = <0x5000 0xeb8>;
					};

					macaddr_lan: macaddr@ffa0 {
						compatible = "mac-base";
						reg = <0xffa0 0x11>;
						#nvmem-cell-cells = <1>;
					};

					macaddr_wan: macaddr@ffb4 {
						compatible = "mac-base";
						reg = <0xffb4 0x11>;
						#nvmem-cell-cells = <1>;
					};
				};
			};

			fwconcat1: partition@670000 {
				label = "fwconcat1";
				reg = <0x670000 0x190000>;
			};
		};
	};
};

&eth0 {
	status = "okay";

	pll-data = <0x11110000 0x00001099 0x00991099>;

	nvmem-cells = <&macaddr_lan 0>;
	nvmem-cell-names = "mac-address";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&eth1 {
	status = "okay";

	pll-data = <0x11110000 0x00001099 0x00991099>;

	nvmem-cells = <&macaddr_wan 0>;
	nvmem-cell-names = "mac-address";

	phy-handle = <&phy4>;
};
