From 7ded2cb303ea93a89b30e1078bc184fb1c05bc68 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.com>
Date: Tue, 11 Mar 2025 08:58:52 +0000
Subject: [PATCH] dts: Remove the power key debounce on Pi 500

Signed-off-by: Phil Elwell <phil@raspberrypi.com>
---
 arch/arm64/boot/dts/broadcom/bcm2712-rpi-500.dts | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm64/boot/dts/broadcom/bcm2712-rpi-500.dts
+++ b/arch/arm64/boot/dts/broadcom/bcm2712-rpi-500.dts
@@ -7,7 +7,7 @@
 };
 
 &pwr_key {
-	debounce-interval = <400>;
+	debounce-interval = <0>;
 };
 
 &gio {
