#include "ar9.dtsi"

#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	compatible = "bt,homehub-v3a", "lantiq,xway", "lantiq,ar9";
	model = "BT Home Hub 3A";  /* SoC: Lantiq ar9 @ 333MHz */

	chosen {
		bootargs = "console=ttyLTQ0,115200";
	};

	aliases {
		led-boot = &power_orange;
		led-failsafe = &power_red;
		led-running = &power_blue;
		led-upgrade = &power_blue;

		led-dsl = &broadband_blue;
		led-wifi = &wireless_blue;
	};

	memory@0 {				  /* RAM: Samsung K4H511638F-LC 64MB */
		device_type = "memory";
		reg = <0x0 0x4000000>;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;
		reset {
			label = "reset";
			gpios = <&gpio 54 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
		restart {
			label = "restart";
			gpios = <&gpio 52 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_POWER>;
		};
		wps {
			label = "wps";
			gpios = <&gpio 53 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};

	leds {
		compatible = "gpio-leds";

		wireless-red {
			label = "red:wireless";
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
		};
		wireless-orange {
			label = "orange:wireless";
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
		};
		wireless_blue: wireless-blue {
			label = "blue:wireless";
			gpios = <&gpio 9 GPIO_ACTIVE_LOW>;
		};

		broadband-red {
			label = "red:broadband";
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
		};
		broadband-orange {
			label = "orange:broadband";
			gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
		};
		broadband_blue: broadband-blue {
			label = "blue:broadband";
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
		};

		power_red: power-red {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_RED>;
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
		};
		power_orange: power-orange {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_ORANGE>;
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};
		power_blue: power-blue {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
		};
	};

	usb_vbus: regulator-usb-vbus {
		compatible = "regulator-fixed";

		regulator-name = "USB_VBUS";

		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;

		gpios = <&gpio 33 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};
};

&gpio {
	pinctrl-names = "default";
	pinctrl-0 = <&state_default>;

	state_default: pinmux {
		pci_rst {
			lantiq,pins = "io21";
			lantiq,output = <1>;
			lantiq,open-drain = <0>;
		};
	};
};

&gsw {
	phy-mode = "rgmii";

	nvmem-cells = <&macaddr_uboot_ethaddr 0>;
	nvmem-cell-names = "mac-address";
};

&ppe {
	nvmem-cells = <&macaddr_uboot_ethaddr 1>;
	nvmem-cell-names = "mac-address";
};

&localbus {
	flash@1 {		  /* NAND Flash: Samsung K9F5608U0D-JIB0 32MB */
		compatible = "lantiq,nand-xway";
		lantiq,cs = <1>;
		bank-width = <2>;
		reg = <1 0x0 0x2000000 >;
		req-mask = <0x1>;  /* PCI request lines to mask during NAND access */

		pinctrl-0 = <&nand_pins>, <&nand_cs1_pins>;
		pinctrl-names = "default";

		nand-use-soft-ecc-engine;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "preboot";
				reg = <0x00000 0x8000>;
				read-only;
			};
			partition@8000 {
				label = "u-boot";
				reg = <0x8000 0x05c000>;
				read-only;
			};
			partition@64000 {
				label = "u-boot-env";
				reg = <0x64000 0x004000>;

				nvmem-layout {
					compatible = "u-boot,env";

					macaddr_uboot_ethaddr: ethaddr {
						#nvmem-cell-cells = <1>;
					};
				};
			};
			ath9k_cal: partition@68000 {
				label = "art-copy";
				reg = <0x68000 0x004000>;
			};
			partition@6c000 {
				label = "kernel";
				reg = <0x6c000 0x200000>;
			};
			partition@26c000 {
				label = "ubi";
				reg = <0x26c000 0x1d94000>;
			};
		};
	};
};

&pci0 {
	status = "okay";

	pinctrl-0 = <&pci_gnt1_pins>, <&pci_req1_pins>;
	pinctrl-names = "default";

	reset-gpios = <&gpio 21 GPIO_ACTIVE_LOW>;

	wifi@e,0 {
		reg = <0x7000 0 0 0 0>;
		qca,no-eeprom; /* load from ath9k-eeprom-pci-0000:00:0e.0.bin */
		nvmem-cells = <&macaddr_uboot_ethaddr 2>;
		nvmem-cell-names = "mac-address";
	};
};

&usb_phy0 {
	status = "okay";
};

&usb0 {
	status = "okay";
	vbus-supply = <&usb_vbus>;
};
