From 70c32664e555b0641cc187eebf0d738eb10a33a0 Mon Sep 17 00:00:00 2001
From: David Plowman <david.plowman@raspberrypi.com>
Date: Tue, 11 May 2021 12:52:26 +0100
Subject: [PATCH] media: i2c: ov5647: Correct pixel array offset

The top offset in the pixel array is actually 6 (see page 3-1 of the
OV5647 data sheet).

Fixes: f2f7ad5ce5e52 ("media: i2c: ov5647: Selection compliance fixes")
Signed-off-by: David Plowman <david.plowman@raspberrypi.com>
---
 drivers/media/i2c/ov5647.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/media/i2c/ov5647.c
+++ b/drivers/media/i2c/ov5647.c
@@ -69,7 +69,7 @@
 #define OV5647_NATIVE_HEIGHT		1956U
 
 #define OV5647_PIXEL_ARRAY_LEFT		16U
-#define OV5647_PIXEL_ARRAY_TOP		16U
+#define OV5647_PIXEL_ARRAY_TOP		6U
 #define OV5647_PIXEL_ARRAY_WIDTH	2592U
 #define OV5647_PIXEL_ARRAY_HEIGHT	1944U
 
