From f7a517f6f1c0ac240e2a2b2bae9c7efb4a92430a Mon Sep 17 00:00:00 2001
From: Robert Marko <robert.marko@sartura.hr>
Date: Tue, 5 Nov 2024 13:36:21 +0100
Subject: [PATCH] reset: sparx5: add LAN969x support

LAN969x uses the same reset configuration as LAN966x, but we need to
allow compiling it when ARCH_LAN969X is selected.

A fallback compatible to LAN966x will be used.

Signed-off-by: Robert Marko <robert.marko@sartura.hr>
---
 drivers/reset/Kconfig | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/reset/Kconfig
+++ b/drivers/reset/Kconfig
@@ -147,7 +147,7 @@ config RESET_LPC18XX
 
 config RESET_MCHP_SPARX5
 	bool "Microchip Sparx5 reset driver"
-	depends on ARCH_SPARX5 || SOC_LAN966 || COMPILE_TEST
+	depends on ARCH_SPARX5 || ARCH_LAN969X || SOC_LAN966 || COMPILE_TEST
 	default y if SPARX5_SWITCH
 	select MFD_SYSCON
 	help
