/* Copyright (c) 2015, The Linux Foundation. All rights reserved.
 * Copyright (c) 2018, David Bauer <mail@david-bauer.net>
 *
 * Permission to use, copy, modify, and/or distribute this software for any
 * purpose with or without fee is hereby granted, provided that the above
 * copyright notice and this permission notice appear in all copies.
 *
 * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
 * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
 * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR
 * ANY SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
 * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN
 * ACTION OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF
 * OR IN CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
 *
 */

#include "qcom-ipq4019.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>
#include <dt-bindings/soc/qcom,tcsr.h>

/ {
	model = "Netgear EX61X0v2";
	compatible = "netgear,ex61x0v2";

	soc {
		tcsr@1949000 {
			compatible = "qcom,tcsr";
			reg = <0x1949000 0x100>;
			qcom,wifi_glb_cfg = <TCSR_WIFI_GLB_CFG>;
		};

		ess_tcsr@1953000 {
			compatible = "qcom,tcsr";
			reg = <0x1953000 0x1000>;
			qcom,ess-interface-select = <TCSR_ESS_PSGMII>;
		};

		tcsr@1957000 {
			compatible = "qcom,tcsr";
			reg = <0x1957000 0x100>;
			qcom,wifi_noc_memtype_m0_m2 = <TCSR_WIFI_NOC_MEMTYPE_M0_M2>;
		};
	};

	aliases {
		// TODO: Verify if the ethernet0 alias is needed
		ethernet0 = &gmac;
		led-boot = &power_amber;
		led-failsafe = &power_amber;
		led-running = &power_green;
		led-upgrade = &power_amber;
		label-mac-device = &gmac;
	};

	keys {
		compatible = "gpio-keys";

		wps {
			label = "wps";
			gpios = <&tlmm 0 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		reset {
			label = "reset";
			gpios = <&tlmm 63 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	led_spi {
		compatible = "spi-gpio";
		#address-cells = <1>;
		#size-cells = <0>;

		sck-gpios = <&tlmm 5 GPIO_ACTIVE_HIGH>;
		mosi-gpios = <&tlmm 4 GPIO_ACTIVE_HIGH>;
		num-chipselects = <0>;

		led_gpio: led_gpio@0 {
			compatible = "fairchild,74hc595";
			reg = <0>;
			gpio-controller;
			#gpio-cells = <2>;
			registers-number = <1>;
			spi-max-frequency = <1000000>;
		};
	};

	leds {
		compatible = "gpio-leds";

		power_amber: power_amber {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_AMBER>;
			gpios = <&led_gpio 7 GPIO_ACTIVE_LOW>;
		};

		power_green: power_green {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&led_gpio 6 GPIO_ACTIVE_LOW>;
		};

		right {
			label = "blue:right";
			gpios = <&led_gpio 5 GPIO_ACTIVE_LOW>;
		};

		left {
			label = "blue:left";
			gpios = <&led_gpio 4 GPIO_ACTIVE_LOW>;
		};

		client_green {
			label = "green:client";
			gpios = <&led_gpio 3 GPIO_ACTIVE_LOW>;
		};

		client_red {
			label = "red:client";
			gpios = <&led_gpio 2 GPIO_ACTIVE_LOW>;
		};

		router_green {
			label = "green:router";
			gpios = <&led_gpio 1 GPIO_ACTIVE_LOW>;
		};

		router_red {
			label = "red:router";
			gpios = <&led_gpio 0 GPIO_ACTIVE_LOW>;
		};

		wps {
			function = LED_FUNCTION_WPS;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&tlmm 1 GPIO_ACTIVE_LOW>;
		};
	};
};

&watchdog {
	status = "okay";
};

&prng {
	status = "okay";
};

&crypto {
	status = "okay";
};

&tlmm {
	serial_pins: serial_pinmux {
		mux {
			pins = "gpio60", "gpio61";
			function = "blsp_uart0";
			bias-disable;
		};
	};

	spi_0_pins: spi_0_pinmux {
		pin {
			function = "blsp_spi0";
			pins = "gpio55", "gpio56", "gpio57";
			drive-strength = <12>;
			bias-disable;
		};
		pin_cs {
			function = "gpio";
			pins = "gpio54";
			drive-strength = <2>;
			bias-disable;
			output-high;
		};
	};
};

&blsp1_spi1 {
	pinctrl-0 = <&spi_0_pins>;
	pinctrl-names = "default";
	status = "okay";
	cs-gpios = <&tlmm 54 GPIO_ACTIVE_LOW>;

	mx25l12805d@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <24000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition0@0 {
				label = "SBL1";
				reg = <0x00000000 0x00040000>;
				read-only;
			};

			partition1@40000 {
				label = "MIBIB";
				reg = <0x00040000 0x00020000>;
				read-only;
			};

			partition2@60000 {
				label = "QSEE";
				reg = <0x00060000 0x00060000>;
				read-only;
			};

			partition3@c0000 {
				label = "CDT";
				reg = <0x000c0000 0x00010000>;
				read-only;
			};

			partition4@d0000 {
				label = "DDRPARAMS";
				reg = <0x000d0000 0x00010000>;
				read-only;
			};

			partition5@E0000 {
				label = "APPSBLENV";
				reg = <0x000e0000 0x00010000>;
				read-only;
			};

			partition6@F0000 {
				label = "APPSBL";
				reg = <0x000f0000 0x00080000>;
				read-only;
			};

			partition7@170000 {
				label = "ART";
				reg = <0x00170000 0x00010000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					precal_art_1000: precal@1000 {
						reg = <0x1000 0x2f20>;
					};

					precal_art_5000: precal@5000 {
						reg = <0x5000 0x2f20>;
					};
				};
			};

			partition8@180000 {
				label = "config";
				reg = <0x00180000 0x00010000>;
				read-only;
			};

			partition9@190000 {
				label = "pot";
				reg = <0x00190000 0x00010000>;
				read-only;
			};

			partition10@1a0000 {
				label = "dnidata";
				reg = <0x001a0000 0x00010000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_dnidata_0: macaddr@0 {
						reg = <0x0 0x6>;
					};

					macaddr_dnidata_c: macaddr@c {
						reg = <0xc 0x6>;
					};
				};
			};

			partition11@1b0000 {
				compatible = "denx,fit";
				label = "firmware";
				reg = <0x001b0000 0x00e10000>;
			};

			partition12@fc0000 {
				label = "language";
				reg = <0x00fc0000 0x00040000>;
				read-only;
			};
		};
	};
};

&blsp1_uart1 {
	pinctrl-0 = <&serial_pins>;
	pinctrl-names = "default";
	status = "okay";
};

&blsp_dma {
	status = "okay";
};

&cryptobam {
	status = "okay";
};

&wifi0 {
	status = "okay";
	nvmem-cell-names = "pre-calibration", "mac-address";
	nvmem-cells = <&precal_art_1000>, <&macaddr_dnidata_0>;
};

&wifi1 {
	status = "okay";
	nvmem-cell-names = "pre-calibration", "mac-address";
	nvmem-cells = <&precal_art_5000>, <&macaddr_dnidata_c>;
};

&mdio {
	status = "okay";
};

&gmac {
	status = "okay";
};

&switch {
	status = "okay";
};

&swport4 {
	status = "okay";
	label = "lan";
};
