From 9aa6ca16f311c4b5d19935167e68731eac8aaeed Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.com>
Date: Mon, 31 Mar 2025 11:49:57 +0100
Subject: [PATCH] overlays: README: Correct "watchdog" default value

The watchdog timer has been enabled by default for a long time now.
Update the documentation for the "watchdog" dtparam to reflect that.

Signed-off-by: Phil Elwell <phil@raspberrypi.com>
---
 arch/arm/boot/dts/overlays/README | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/arch/arm/boot/dts/overlays/README
+++ b/arch/arm/boot/dts/overlays/README
@@ -463,8 +463,8 @@ Params:
         uart1                   Set to "on" or "off" to enable or disable uart1
                                 (default varies)
 
-        watchdog                Set to "on" to enable the hardware watchdog
-                                (default "off")
+        watchdog                Set to "off" to disable the hardware watchdog
+                                (default "on")
 
         wifiaddr                Set an alternative WiFi MAC address.
                                 The value should be a 6-byte hexadecimal value,
