#include "vr9.dtsi"

#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>
#include <dt-bindings/mips/lantiq_rcu_gphy.h>

/ {
	compatible = "zyxel,p-2812hnu", "lantiq,xway", "lantiq,vr9";

	chosen {
		bootargs = "console=ttyLTQ0,115200";
	};

	aliases {
		led-boot = &power_green;
		led-failsafe = &power_red;
		led-running = &power_green;
		led-upgrade = &power_green;

		led-dsl = &dsl_green;
		led-internet = &internet_green;
		led-wifi = &wireless_green;
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x8000000>;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;

		reset {
			label = "reset";
			gpios = <&gpio 39 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		rfkill {
			label = "rfkill";
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RFKILL>;
		};
	};

	leds {
		compatible = "gpio-leds";

		internet_red {
			label = "red:internet";
			gpios = <&stp 16 GPIO_ACTIVE_LOW>;
		};
		internet_green: internet_green {
			label = "green:internet";
			gpios = <&stp 17 GPIO_ACTIVE_LOW>;
		};
		dsl_green: dsl_green {
			label = "green:dsl";
			gpios = <&stp 18 GPIO_ACTIVE_LOW>;
		};
		dsl_orange {
			label = "orange:dsl";
			gpios = <&stp 19 GPIO_ACTIVE_LOW>;
		};
		wireless_orange {
			function = LED_FUNCTION_WLAN;
			color = <LED_COLOR_ID_ORANGE>;
			gpios = <&stp 20 GPIO_ACTIVE_LOW>;
		};
		wireless_green: wireless_green {
			function = LED_FUNCTION_WLAN;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&stp 21 GPIO_ACTIVE_LOW>;
		};
		power_red: power {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_RED>;
			gpios = <&stp 22 GPIO_ACTIVE_LOW>;
		};
		power_green: power2 {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&stp 23 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};
		phone1 {
			label = "green:phone";
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
		};
		phone1warn {
			label = "orange:phone";
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
		};
		phone2warn {
			label = "orange:phone2";
			gpios = <&gpio 26 GPIO_ACTIVE_LOW>;
		};
		phone2 {
			label = "green:phone2";
			gpios = <&gpio 28 GPIO_ACTIVE_LOW>;
		};
	};

	usb_vbus: regulator-usb-vbus {
		compatible = "regulator-fixed";

		regulator-name = "USB_VBUS";

		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;

		gpios = <&gpio 33 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};
};

&gphy0 {
	lantiq,gphy-mode = <GPHY_MODE_GE>;
};

&gphy1 {
	lantiq,gphy-mode = <GPHY_MODE_GE>;
};

&gpio {
	pinctrl-names = "default";
	pinctrl-0 = <&state_default>;

	state_default: pinmux {
		exin3 {
			lantiq,groups = "exin3";
			lantiq,function = "exin";
		};
		pci_rst {
			lantiq,pins = "io21";
			lantiq,output = <1>;
			lantiq,open-drain = <0>;
			lantiq,pull = <2>;
		};
		pcie-rst {
			lantiq,pins = "io38";
			lantiq,pull = <0>;
			lantiq,output = <1>;
		};
		ifxhcd-rst {
			lantiq,pins = "io33";
			lantiq,pull = <0>;
			lantiq,open-drain = <0>;
			lantiq,output = <1>;
		};
	};
};

&gswip {
	pinctrl-0 = <&mdio_pins>,
		    <&gphy0_led1_pins>, <&gphy0_led2_pins>,
		    <&gphy1_led1_pins>, <&gphy1_led2_pins>;
	pinctrl-names = "default";
	nvmem-cells = <&macaddr_uboot_ethaddr 0>;
	nvmem-cell-names = "mac-address";
};

&gswip_mdio {
	phy0: ethernet-phy@0 {
		reg = <0x0>;
	};
	phy1: ethernet-phy@1 {
		reg = <0x1>;
	};
	phy5: ethernet-phy@5 {
		reg = <0x5>;
	};
	phy11: ethernet-phy@11 {
		reg = <0x11>;
	};
	phy13: ethernet-phy@13 {
		reg = <0x13>;
	};
};

&gswip_ports {
	port@0 {
		reg = <0>;
		label = "lan1";
		phy-mode = "rgmii";
		phy-handle = <&phy0>;
	};
	port@1 {
		reg = <1>;
		label = "lan2";
		phy-mode = "rgmii";
		phy-handle = <&phy1>;
	};
	port@2 {
		reg = <2>;
		label = "lan3";
		phy-mode = "internal";
		phy-handle = <&phy11>;
	};
	port@4 {
		reg = <4>;
		label = "lan4";
		phy-mode = "internal";
		phy-handle = <&phy13>;
	};
	port@5 {
		reg = <5>;
		label = "wan";
		phy-mode = "rgmii";
		phy-handle = <&phy5>;
		nvmem-cells = <&macaddr_uboot_ethaddr 1>;
		nvmem-cell-names = "mac-address";
	};
};

&pci0 {
	status = "okay";

	pinctrl-0 = <&pci_gnt1_pins>, <&pci_req1_pins>;
	pinctrl-names = "default";

	reset-gpios = <&gpio 21 GPIO_ACTIVE_LOW>;
};

&stp {
	status = "okay";
};

&usb_phy0 {
	status = "okay";
};

&usb_phy1 {
	status = "okay";
};

&usb0 {
	status = "okay";
	vbus-supply = <&usb_vbus>;
};

&usb1 {
	status = "okay";
	vbus-supply = <&usb_vbus>;
};
