From e5f25e25ed6c0478cbba7a32891b911e3183dad4 Mon Sep 17 00:00:00 2001
From: Lars-Peter Clausen <lars@metafoo.de>
Date: Wed, 13 Oct 2010 01:17:24 +0200
Subject: [PATCH 08/21] qi_lb60: Don't use 3-wire spi mode for the display for
 now

The spi_gpio driver does not support 3-wire mode.
---
 arch/mips/jz4740/board-qi_lb60.c |    1 -
 1 files changed, 0 insertions(+), 1 deletions(-)

--- a/arch/mips/jz4740/board-qi_lb60.c
+++ b/arch/mips/jz4740/board-qi_lb60.c
@@ -310,7 +310,6 @@ static struct spi_board_info qi_lb60_spi
 		.chip_select = 0,
 		.bus_num = 1,
 		.max_speed_hz = 30 * 1000,
-		.mode = SPI_3WIRE,
 	},
 };
 
