--- a/drivers/net/wireless/ath/ath9k/ar9003_phy.c
+++ b/drivers/net/wireless/ath/ath9k/ar9003_phy.c
@@ -1085,6 +1085,10 @@ static bool ar9003_hw_ani_control(struct
 		 * is_on == 0 means MRC CCK is OFF (more noise imm)
 		 */
 		bool is_on = param ? 1 : 0;
+
+		if (ah->caps.rx_chainmask == 1)
+			break;
+
 		REG_RMW_FIELD(ah, AR_PHY_MRC_CCK_CTRL,
 			      AR_PHY_MRC_CCK_ENABLE, is_on);
 		REG_RMW_FIELD(ah, AR_PHY_MRC_CCK_CTRL,
