--- a/drivers/leds/Kconfig
+++ b/drivers/leds/Kconfig
@@ -453,6 +453,13 @@ config LEDS_TRIGGERS
 	  These triggers allow kernel events to drive the LEDs and can
 	  be configured via sysfs. If unsure, say Y.
 
+config LEDS_WNDR3700_USB
+	tristate "NETGEAR WNDR3700 USB LED driver"
+	depends on LEDS_CLASS && ATH79_MACH_WNDR3700
+	help
+	  This option enables support for the USB LED found on the
+	  NETGEAR WNDR3700 board.
+
 comment "LED Triggers"
 
 config LEDS_TRIGGER_TIMER
--- a/drivers/leds/Makefile
+++ b/drivers/leds/Makefile
@@ -37,6 +37,7 @@ obj-$(CONFIG_LEDS_DA9052)		+= leds-da905
 obj-$(CONFIG_LEDS_WM831X_STATUS)	+= leds-wm831x-status.o
 obj-$(CONFIG_LEDS_WM8350)		+= leds-wm8350.o
 obj-$(CONFIG_LEDS_PWM)			+= leds-pwm.o
+obj-${CONFIG_LEDS_WNDR3700_USB}		+= leds-wndr3700-usb.o
 obj-$(CONFIG_LEDS_REGULATOR)		+= leds-regulator.o
 obj-$(CONFIG_LEDS_INTEL_SS4200)		+= leds-ss4200.o
 obj-$(CONFIG_LEDS_LT3593)		+= leds-lt3593.o
