From e79bc74f76361020d820ed4611d28f70ebd845ca Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jonas.gorski@gmail.com>
Date: Tue, 10 Jul 2012 10:44:09 +0200
Subject: [PATCH 34/84] bcm63xx_enet: don't overwrite settings when setting duplex on force

---
 drivers/net/ethernet/broadcom/bcm63xx_enet.c |    2 +-
 1 files changed, 1 insertions(+), 1 deletions(-)

--- a/drivers/net/ethernet/broadcom/bcm63xx_enet.c
+++ b/drivers/net/ethernet/broadcom/bcm63xx_enet.c
@@ -2333,7 +2333,7 @@ static int bcm_enetsw_open(struct net_de
 		}
 
 		if (port->force_duplex_full)
-			override = ENETSW_IMPOV_FDX_MASK;
+			override |= ENETSW_IMPOV_FDX_MASK;
 
 
 		enetsw_writeb(priv, override, ENETSW_PORTOV_REG(i));
