From 04216bedafb1b3992a6c2b7f1518281d2ba5fc7b Mon Sep 17 00:00:00 2001
From: Kuninori Morimoto <kuninori.morimoto.gx@renesas.com>
Date: Mon, 6 Aug 2012 18:08:39 -0700
Subject: [PATCH] usb: host: ehci-platform: add platform specific power callback

Commit 04216bedafb1b3992a6c2b7f1518281d2ba5fc7b upstream.

This patch enables to call platform specific power callback function.

Signed-off-by: Kuninori Morimoto <kuninori.morimoto.gx@renesas.com>
Acked-by: Alan Stern <stern@rowland.harvard.edu>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/usb/host/ehci-platform.c |   40 +++++++++++++++++++++++++++++++++++---
 include/linux/usb/ehci_pdriver.h |    8 ++++++++
 2 files changed, 45 insertions(+), 3 deletions(-)

--- a/drivers/usb/host/ehci-platform.c
+++ b/drivers/usb/host/ehci-platform.c
@@ -105,10 +105,18 @@ static int __devinit ehci_platform_probe
 		return -ENXIO;
 	}
 
+	if (pdata->power_on) {
+		err = pdata->power_on(dev);
+		if (err < 0)
+			return err;
+	}
+
 	hcd = usb_create_hcd(&ehci_platform_hc_driver, &dev->dev,
 			     dev_name(&dev->dev));
-	if (!hcd)
-		return -ENOMEM;
+	if (!hcd) {
+		err = -ENOMEM;
+		goto err_power;
+	}
 
 	hcd->rsrc_start = res_mem->start;
 	hcd->rsrc_len = resource_size(res_mem);
@@ -136,12 +144,17 @@ err_release_region:
 	release_mem_region(hcd->rsrc_start, hcd->rsrc_len);
 err_put_hcd:
 	usb_put_hcd(hcd);
+err_power:
+	if (pdata->power_off)
+		pdata->power_off(dev);
+
 	return err;
 }
 
 static int __devexit ehci_platform_remove(struct platform_device *dev)
 {
 	struct usb_hcd *hcd = platform_get_drvdata(dev);
+	struct usb_ehci_pdata *pdata = dev->dev.platform_data;
 
 	usb_remove_hcd(hcd);
 	iounmap(hcd->regs);
@@ -149,6 +162,9 @@ static int __devexit ehci_platform_remov
 	usb_put_hcd(hcd);
 	platform_set_drvdata(dev, NULL);
 
+	if (pdata->power_off)
+		pdata->power_off(dev);
+
 	return 0;
 }
 
@@ -157,14 +173,32 @@ static int __devexit ehci_platform_remov
 static int ehci_platform_suspend(struct device *dev)
 {
 	struct usb_hcd *hcd = dev_get_drvdata(dev);
+	struct usb_ehci_pdata *pdata = dev->platform_data;
+	struct platform_device *pdev =
+		container_of(dev, struct platform_device, dev);
 	bool do_wakeup = device_may_wakeup(dev);
+	int ret;
+
+	ret = ehci_suspend(hcd, do_wakeup);
 
-	return ehci_suspend(hcd, do_wakeup);
+	if (pdata->power_suspend)
+		pdata->power_suspend(pdev);
+
+	return ret;
 }
 
 static int ehci_platform_resume(struct device *dev)
 {
 	struct usb_hcd *hcd = dev_get_drvdata(dev);
+	struct usb_ehci_pdata *pdata = dev->platform_data;
+	struct platform_device *pdev =
+		container_of(dev, struct platform_device, dev);
+
+	if (pdata->power_on) {
+		int err = pdata->power_on(pdev);
+		if (err < 0)
+			return err;
+	}
 
 	ehci_resume(hcd, false);
 	return 0;
--- a/include/linux/usb/ehci_pdriver.h
+++ b/include/linux/usb/ehci_pdriver.h
@@ -41,6 +41,14 @@ struct usb_ehci_pdata {
 	unsigned	big_endian_mmio:1;
 	unsigned	port_power_on:1;
 	unsigned	port_power_off:1;
+
+	/* Turn on all power and clocks */
+	int (*power_on)(struct platform_device *pdev);
+	/* Turn off all power and clocks */
+	void (*power_off)(struct platform_device *pdev);
+	/* Turn on only VBUS suspend power and hotplug detection,
+	 * turn off everything else */
+	void (*power_suspend)(struct platform_device *pdev);
 };
 
 #endif /* __USB_CORE_EHCI_PDRIVER_H */
