From f7d7b362b51c51c1ae80bb7ade2039d6f74d4070 Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Sun, 24 Jun 2012 13:46:26 +0200
Subject: [PATCH 22/34] MIPS: ath79: register UART for the QCA955X SoCs

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>
---
 arch/mips/ath79/dev-common.c |    3 ++-
 1 files changed, 2 insertions(+), 1 deletions(-)

--- a/arch/mips/ath79/dev-common.c
+++ b/arch/mips/ath79/dev-common.c
@@ -90,7 +90,8 @@ void __init ath79_register_uart(void)
 	if (soc_is_ar71xx() ||
 	    soc_is_ar724x() ||
 	    soc_is_ar913x() ||
-	    soc_is_ar934x()) {
+	    soc_is_ar934x() ||
+	    soc_is_qca955x()) {
 		ath79_uart_data[0].uartclk = clk_get_rate(clk);
 		platform_device_register(&ath79_uart_device);
 	} else if (soc_is_ar933x()) {
