--- a/drivers/net/phy/Kconfig
+++ b/drivers/net/phy/Kconfig
@@ -140,6 +140,11 @@ config RTL8306_PHY
 	tristate "Driver for Realtek RTL8306S switches"
 	select SWCONFIG
 
+config MICREL_PHY
+	tristate "Drivers for Micrel/Kendin PHYs"
+	---help---
+	  Currently has a driver for the KSZ8041
+
 config FIXED_PHY
 	bool "Driver for MDIO Bus/PHY emulation with fixed speed/link PHYs"
 	depends on PHYLIB=y
--- a/drivers/net/phy/Makefile
+++ b/drivers/net/phy/Makefile
@@ -28,6 +28,7 @@ obj-$(CONFIG_RTL8366S_PHY)	+= rtl8366s.o
 obj-$(CONFIG_RTL8366RB_PHY)	+= rtl8366rb.o
 obj-$(CONFIG_RTL8367_PHY)	+= rtl8367.o
 obj-$(CONFIG_LSI_ET1011C_PHY)	+= et1011c.o
+obj-$(CONFIG_MICREL_PHY)	+= micrel.o
 obj-$(CONFIG_FIXED_PHY)		+= fixed.o
 obj-$(CONFIG_MDIO_BITBANG)	+= mdio-bitbang.o
 obj-$(CONFIG_MDIO_GPIO)		+= mdio-gpio.o
