From e0095e21dd9179250c304d6df2643e9a50d48edb Mon Sep 17 00:00:00 2001
From: Christian Marangi <ansuelsmth@gmail.com>
Date: Fri, 7 Feb 2025 13:25:28 +0100
Subject: [PATCH 05/10] dt-bindings: phy: Add documentation for Airoha AN7581
 USB PHY

Add documentation for Airoha AN7581 USB PHY that describe the USB PHY
for the USB controller.

Airoha AN7581 SoC support a maximum of 2 USB port. The USB 2.0 mode is
always supported. The USB 3.0 mode is optional and depends on the Serdes
mode currently configured on the system for the USB port.

If the airoha,serdes-port property is not declared, it's assumed USB 3.0
mode is not supported, as the Serdes mode can't be validated.

Signed-off-by: Christian Marangi <ansuelsmth@gmail.com>
---
 .../bindings/phy/airoha,an7581-usb-phy.yaml   | 83 +++++++++++++++++++
 MAINTAINERS                                   |  7 ++
 .../dt-bindings/phy/airoha,an7581-usb-phy.h   | 11 +++
 3 files changed, 101 insertions(+)
 create mode 100644 Documentation/devicetree/bindings/phy/airoha,an7581-usb-phy.yaml
 create mode 100644 include/dt-bindings/phy/airoha,an7581-usb-phy.h

--- /dev/null
+++ b/Documentation/devicetree/bindings/phy/airoha,an7581-usb-phy.yaml
@@ -0,0 +1,83 @@
+# SPDX-License-Identifier: GPL-2.0-only OR BSD-2-Clause
+%YAML 1.2
+---
+$id: http://devicetree.org/schemas/phy/airoha,an7581-usb-phy.yaml#
+$schema: http://devicetree.org/meta-schemas/core.yaml#
+
+title: Airoha AN7581 SoC USB PHY
+
+maintainers:
+  - Christian Marangi <ansuelsmth@gmail.com>
+
+description: >
+  The Airoha AN7581 SoC USB PHY describes the USB PHY for the USB controller.
+
+  Airoha AN7581 SoC support a maximum of 2 USB port. The USB 2.0 mode is
+  always supported. The USB 3.0 mode is optional and depends on the Serdes
+  mode currently configured on the system for the USB port.
+
+  If the airoha,serdes-port property is not declared, it's assumed USB 3.0
+  mode is not supported, as the Serdes mode can't be validated.
+
+properties:
+  compatible:
+    const: airoha,an7581-usb-phy
+
+  reg:
+    maxItems: 1
+
+
+  airoha,usb2-monitor-clk-sel:
+    description: Describe what oscillator across the available 4
+      should be selected for USB 2.0 Slew Rate calibration.
+    $ref: /schemas/types.yaml#/definitions/uint32
+    enum: [0, 1, 2, 3]
+
+  airoha,serdes-port:
+    description: Describe what Serdes Port is attached to the USB 3.0 port.
+    $ref: /schemas/types.yaml#/definitions/uint32
+    enum: [0, 1, 2, 3]
+
+  airoha,scu:
+    description: Phandle to the SCU node for USB 3.0 Serdes mode validation.
+    $ref: /schemas/types.yaml#/definitions/phandle
+
+  '#phy-cells':
+    const: 1
+
+required:
+  - compatible
+  - reg
+  - airoha,usb2-monitor-clk-sel
+  - '#phy-cells'
+
+dependentRequired:
+  airoha,serdes-port: [ 'airoha,scu' ]
+
+additionalProperties: false
+
+examples:
+  - |
+    #include <dt-bindings/phy/airoha,an7581-usb-phy.h>
+    #include <dt-bindings/soc/airoha,scu-ssr.h>
+
+    phy@1fac0000 {
+        compatible = "airoha,an7581-usb-phy";
+        reg = <0x1fac0000 0x10000>;
+
+        airoha,usb2-monitor-clk-sel = <AIROHA_USB2_MONCLK_SEL1>;
+        airoha,scu = <&scu>;
+        airoha,serdes-port = <AIROHA_SCU_SERDES_USB1>;
+
+        #phy-cells = <1>;
+    };
+
+    phy@1fae0000 {
+        compatible = "airoha,an7581-usb-phy";
+        reg = <0x1fae0000 0x10000>;
+
+        airoha,usb2-monitor-clk-sel = <AIROHA_USB2_MONCLK_SEL2>;
+
+        #phy-cells = <1>;
+    };
+
--- a/MAINTAINERS
+++ b/MAINTAINERS
@@ -745,6 +745,13 @@ S:	Maintained
 F:	Documentation/devicetree/bindings/spi/airoha,en7581-snand.yaml
 F:	drivers/spi/spi-airoha-snfi.c
 
+AIROHA USB PHY DRIVER
+M:	Christian Marangi <ansuelsmth@gmail.com>
+L:	linux-arm-kernel@lists.infradead.org (moderated for non-subscribers)
+S:	Maintained
+F:	Documentation/devicetree/bindings/phy/airoha,an7581-usb-phy.yaml
+F:	include/dt-bindings/phy/airoha,an7581-usb-phy.h
+
 AIRSPY MEDIA DRIVER
 L:	linux-media@vger.kernel.org
 S:	Orphan
--- /dev/null
+++ b/include/dt-bindings/phy/airoha,an7581-usb-phy.h
@@ -0,0 +1,11 @@
+/* SPDX-License-Identifier: GPL-2.0-only OR BSD-2-Clause */
+
+#ifndef _DT_BINDINGS_AIROHA_AN7581_USB_PHY_H_
+#define _DT_BINDINGS_AIROHA_AN7581_USB_PHY_H_
+
+#define AIROHA_USB2_MONCLK_SEL0                 0
+#define AIROHA_USB2_MONCLK_SEL1                 1
+#define AIROHA_USB2_MONCLK_SEL2                 2
+#define AIROHA_USB2_MONCLK_SEL3                 3
+
+#endif
