From 41742f746f4860ad7658484ec24a2971476a9d05 Mon Sep 17 00:00:00 2001
From: Daniel Machon <daniel.machon@microchip.com>
Date: Fri, 1 Nov 2024 08:09:10 +0100
Subject: [PATCH 61/82] net: sparx5: execute sparx5_vcap_init() on lan969x
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

The is_sparx5() check was introduced in an earlier series, to make sure
the sparx5_vcap_init() was not executed on lan969x, as it was not
implemented there yet. Now that it is, remove that check.

Reviewed-by: Steen Hegelund <Steen.Hegelund@microchip.com>
Reviewed-by: Jens Emil Schulz Østergaard <jensemil.schulzostergaard@microchip.com>
Signed-off-by: Daniel Machon <daniel.machon@microchip.com>
Signed-off-by: Paolo Abeni <pabeni@redhat.com>
---
 drivers/net/ethernet/microchip/sparx5/sparx5_main.c | 10 ++++------
 1 file changed, 4 insertions(+), 6 deletions(-)

--- a/drivers/net/ethernet/microchip/sparx5/sparx5_main.c
+++ b/drivers/net/ethernet/microchip/sparx5/sparx5_main.c
@@ -770,12 +770,10 @@ static int sparx5_start(struct sparx5 *s
 	if (err)
 		return err;
 
-	if (is_sparx5(sparx5)) {
-		err = sparx5_vcap_init(sparx5);
-		if (err) {
-			sparx5_unregister_notifier_blocks(sparx5);
-			return err;
-		}
+	err = sparx5_vcap_init(sparx5);
+	if (err) {
+		sparx5_unregister_notifier_blocks(sparx5);
+		return err;
 	}
 
 	/* Start Frame DMA with fallback to register based INJ/XTR */
