From 22fb5991a44c78ff18ec0082dc90c809356eb893 Mon Sep 17 00:00:00 2001
From: Ansuel Smith <ansuelsmth@gmail.com>
Date: Sun, 27 Sep 2020 19:23:35 +0200
Subject: [PATCH 1/2] ath10k: Try to get mac-address from dts

Most of embedded device that have the ath10k wifi integrated store the
mac-address in nvmem partitions. Try to fetch the mac-address using the
standard 'of_get_mac_address' than in all the check also try to fetch the
address using the nvmem api searching for a defined 'mac-address' cell.
Mac-address defined in the dts have priority than any other address found.

Tested-on: QCA9984 hw1.0 PCI 10.4

Signed-off-by: Ansuel Smith <ansuelsmth@gmail.com>
---
 drivers/net/wireless/ath/ath10k/core.c | 10 ++++++++++
 1 file changed, 10 insertions(+)

--- a/drivers/net/wireless/ath/ath10k/core.c
+++ b/drivers/net/wireless/ath/ath10k/core.c
@@ -11,6 +11,7 @@
 #include <linux/module.h>
 #include <linux/firmware.h>
 #include <linux/of.h>
+#include <linux/of_net.h>
 #include <linux/property.h>
 #include <linux/dmi.h>
 #include <linux/ctype.h>
@@ -3458,6 +3459,8 @@ static int ath10k_core_probe_fw(struct a
 
 	device_get_mac_address(ar->dev, ar->mac_addr);
 
+	of_get_mac_address(ar->dev->of_node, ar->mac_addr);
+
 	ret = ath10k_core_init_firmware_features(ar);
 	if (ret) {
 		ath10k_err(ar, "fatal problem with firmware features: %d\n",
