From 6f268e275c74dae0536e0b61982a8db25bcf4f16 Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jonas.gorski@gmail.com>
Date: Fri, 28 Nov 2025 09:06:19 +0100
Subject: [PATCH] net: dsa: b53: fix VLAN_ID_IDX write size for BCM5325/65
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Since BCM5325 and BCM5365 only support up to 256 VLANs, the VLAN_ID_IDX
register is only 8 bit wide, not 16 bit, so use an appropriate accessor.

Fixes: c45655386e53 ("net: dsa: b53: add support for FDB operations on 5325/5365")
Reviewed-by: Florian Fainelli <florian.fainelli@broadcom.com>
Tested-by: Álvaro Fernández Rojas <noltari@gmail.com>
Signed-off-by: Jonas Gorski <jonas.gorski@gmail.com>
Link: https://patch.msgid.link/20251128080625.27181-2-jonas.gorski@gmail.com
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/dsa/b53/b53_common.c | 8 ++++++--
 1 file changed, 6 insertions(+), 2 deletions(-)

--- a/drivers/net/dsa/b53/b53_common.c
+++ b/drivers/net/dsa/b53/b53_common.c
@@ -1946,8 +1946,12 @@ static int b53_arl_op(struct b53_device
 
 	/* Perform a read for the given MAC and VID */
 	b53_write48(dev, B53_ARLIO_PAGE, B53_MAC_ADDR_IDX, mac);
-	if (!is5325m(dev))
-		b53_write16(dev, B53_ARLIO_PAGE, B53_VLAN_ID_IDX, vid);
+	if (!is5325m(dev)) {
+		if (is5325(dev) || is5365(dev))
+			b53_write8(dev, B53_ARLIO_PAGE, B53_VLAN_ID_IDX, vid);
+		else
+			b53_write16(dev, B53_ARLIO_PAGE, B53_VLAN_ID_IDX, vid);
+	}
 
 	/* Issue a read operation for this MAC */
 	ret = b53_arl_rw_op(dev, 1);
