From: Christian Marangi <ansuelsmth@gmail.com>
Subject: kernel/mtd: add support for EON EN25QX128A

Add support for EON EN25QX128A with no flags as it does
support SFDP parsing.

Signed-off-by: Christian Marangi <ansuelsmth@gmail.com>
---
 drivers/mtd/spi-nor/spi-nor.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/mtd/spi-nor/eon.c
+++ b/drivers/mtd/spi-nor/eon.c
@@ -23,6 +23,10 @@ static const struct flash_info eon_nor_p
 		.size = SZ_16M,
 		.no_sfdp_flags = SECT_4K,
 	}, {
+		.id = SNOR_ID(0x1c, 0x71, 0x18),
+		.name = "en25qx128a",
+		.size = SZ_16M,
+	}, {
 		.id = SNOR_ID(0x1c, 0x30, 0x14),
 		.name = "en25q80a",
 		.size = SZ_1M,
