// SPDX-License-Identifier: GPL-2.0-or-later

#include "bcm6358.dtsi"

/ {
	model = "Huawei EchoLife HG556a (version B)";
	compatible = "huawei,hg556a-b", "brcm,bcm6358";

	aliases {
		led-boot = &led_power_red;
		led-failsafe = &led_power_red;
		led-running = &led_power_red;
		led-upgrade = &led_power_red;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;

		help {
			label = "help";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_HELP>;
			debounce-interval = <60>;
		};

		wlan {
			label = "wlan";
			gpios = <&gpio 9 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WLAN>;
			debounce-interval = <60>;
		};

		restart {
			label = "restart";
			gpios = <&gpio 10 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
		};

		reset {
			label = "reset";
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_CONFIG>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led-0 {
			label = "red:message";
			gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
		};

		led-1 {
			label = "red:hspa";
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
		};

		led-2 {
			label = "red:dsl";
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
		};

		led_power_red: led-3 {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_RED>;
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
		};

		led-6 {
			label = "all";
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		led-12 {
			label = "green:lan1";
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
		};

		led-13 {
			label = "red:lan1";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
		};

		led-15 {
			label = "green:lan2";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};

		led-22 {
			label = "red:lan2";
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
		};

		led-23 {
			label = "green:lan3";
			gpios = <&gpio 23 GPIO_ACTIVE_LOW>;
		};

		led-26 {
			label = "red:lan3";
			gpios = <&gpio 26 GPIO_ACTIVE_LOW>;
		};

		led-27 {
			label = "green:lan4";
			gpios = <&gpio 27 GPIO_ACTIVE_LOW>;
		};

		led-28 {
			label = "red:lan4";
			gpios = <&gpio 28 GPIO_ACTIVE_LOW>;
		};
	};

	ath9k-leds {
		compatible = "gpio-leds";

		led-2 {
			function = LED_FUNCTION_WLAN;
			color = <LED_COLOR_ID_RED>;
			gpios = <&ath9k 2 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "phy0tpt";
		};
	};
};

&ehci {
	status = "okay";
};

&ethernet1 {
	status = "okay";

	nvmem-cells = <&macaddr_cfe_6a0 0>;
	nvmem-cell-names = "mac-address";

	phy-mode = "mii";

	fixed-link {
		speed = <100>;
		full-duplex;
	};
};

&iudma {
	status = "okay";
};

&ohci {
	status = "okay";
};

&pci {
	status = "okay";

	ath9k: wifi@1,0 {
		compatible = "pci168c,0029";
		reg = <0x0800 0 0 0 0>;

		qca,no-eeprom;

		nvmem-cells = <&macaddr_cfe_6a0 1>;
		nvmem-cell-names = "mac-address";

		#gpio-cells = <2>;
		gpio-controller;
	};
};

&pflash {
	status = "okay";

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		partition@0 {
			label = "cfe";
			reg = <0x000000 0x020000>;
			read-only;

			nvmem-layout {
				compatible = "fixed-layout";
				#address-cells = <1>;
				#size-cells = <1>;

				macaddr_cfe_6a0: macaddr@6a0 {
					compatible = "mac-base";
					reg = <0x6a0 0x6>;
					#nvmem-cell-cells = <1>;
				};
			};
		};

		partition@20000 {
			label = "firmware";
			reg = <0x020000 0xec0000>;
			compatible = "brcm,bcm963xx-imagetag";
		};

		cal_data: partition@ee0000 {
			label = "cal_data";
			reg = <0xee0000 0x100000>;
			read-only;

			nvmem-layout {
				compatible = "fixed-layout";
				#address-cells = <1>;
				#size-cells = <1>;

				cal_data_1e000: cal@1e000 {
					reg = <0x1e000 0xeb8>;
				};
			};
		};

		partition@fe0000 {
			label = "nvram";
			reg = <0xfe0000 0x020000>;
		};
	};
};

&uart0 {
	status = "okay";
};

&usbh {
	status = "okay";
};
