From 9c059700fee595142676a9bbaff6e40e3fcd9cbb Mon Sep 17 00:00:00 2001
From: Sebastian Reichel <sebastian.reichel@collabora.com>
Date: Mon, 18 Aug 2025 19:18:40 +0200
Subject: [PATCH] arm64: dts: rockchip: Enable RK3576 watchdog

The RK3576 watchdog does not need any board specific resources, so
let's enable it by default just like we do for RK3588.

Signed-off-by: Sebastian Reichel <sebastian.reichel@collabora.com>
Link: https://lore.kernel.org/r/20250818-rk3576-watchdog-v1-1-28f82e01029c@kernel.org
Signed-off-by: Heiko Stuebner <heiko@sntech.de>
---
 arch/arm64/boot/dts/rockchip/rk3576.dtsi | 1 -
 1 file changed, 1 deletion(-)

--- a/arch/arm64/boot/dts/rockchip/rk3576.dtsi
+++ b/arch/arm64/boot/dts/rockchip/rk3576.dtsi
@@ -2275,7 +2275,6 @@
 			clocks = <&cru TCLK_WDT0>, <&cru PCLK_WDT0>;
 			clock-names = "tclk", "pclk";
 			interrupts = <GIC_SPI 40 IRQ_TYPE_LEVEL_HIGH>;
-			status = "disabled";
 		};
 
 		spi0: spi@2acf0000 {
