#config driver 'upsname'
#	option driver usbhid-ups
#	option port auto
#	option other other-value
#	option runas root

#config user
#	option username upsuser
#	option password upspassword
#	option actions optional-action
#	list instcmd optional-instant-command
#	option upsmon slave|master

#config listen_address
#	option address ::1
#	option port 3493

#config upsd 'upsd'
#	option maxage 15
#	option statepath /var/run/nut
#	option maxconn 1024
#	option runas nut
# NB: certificates only apply to SSL-enabled version
#       option certfile /usr/local/etc/upsd.pem
